
                           List of USA TV Limitations                           
2015/08/31                                                             Page:   1
                                                                                
                                                                                
                                                                                

 Code Limitation                                                                
----- ----------------------------------------------------------------------    
    1 Limitation to protect Edmundston, N.B.                                    
    2 Limited to 100 kW maximum ERP and 305 m EHAAT, or the equivalent, in      
      the general direction of Brandon, Man.                                    
                                                                                
    3 Limited to protect CBFT Montreal signal at Canada-U.S.A. border.          
    4 Limitation to protect Channel 62 Shediac, NB.                             
    5 Limitation of 20 dBk at 305m  EHAAT.                                      
    6 Limited to 1 kW ERP and 390 m HAAT or equivalent towards ch. 23 B         
      (DTV) in Sault Ste. Marie, ON.                                            
                                                                                
    7 Limited to 500 kW ERP and 287 m HAAT or equivalent towards ch. 33 DTV     
      in Barrie, ON.                                                            
                                                                                
    8 -13 DB TO 15DTV DIGBY, NS                                                 
    9 -7 DB TO 22DTV SAINT JOHN, NB                                             
   10 -3 DB TO 53DTV TORONTO, ON                                                
   11 -3 DB TO 33DTV BARRIE, ON                                                 
   12 -20 DB TO 34DTV PETERBOROUGH, ON                                          
   13 Limited to 5 kW at 150 m or equivalent                                    
   14 Limited to 443 kW at 845.2 m or equivalent.  ERP may be increased to      
      550 kW when channel 22 DTV in Ottawa, ON goes to post-transition class    
      VL parameters.                                                            
                                                                                

14 rows selected.

